{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":28,"n_cols":4,"rows_kept":28,"cut":false,"hidden":false,"merged":[[3,1,3,3],[5,1,5,3],[7,1,7,3],[10,1,10,3],[14,1,14,3],[21,1,21,3],[26,1,26,3],[3,0,27,0],[0,0,1,3]]}
["3行C列开始填入车型类别\n具体参数请按下方案例编辑、填入"]
[]
[null,null,"AUMAN Galaxy 660PS 6X4 tractor1","AUMAN Galaxy 660PS 6X4 tractor2"]
["技术参数 Specifications","驾驶室形式 Cab boby type"]
[null,"驾驶室形式 Cab boby type","银河高顶高地板 Galaxy high roof&high floc","银河高顶高地板 Galaxy high roof&high floc"]
[null,"驱动 Drive style"]
[null,"驱动 Drive style","6x4","6x4"]
[null,"尺寸参数 Dimension"]
[null,"整车外形尺寸(长x宽x高,mm) Overall dimensions (LxWx H.mm)","7115x2525x3950","7115x2525x3950"]
[null,"轴距(mm) Wheelbase(mm)","3300+1350","3300+1350"]
[null,"重量参数 Mass"]
[null,"最大设计重量(kg) Maximum Gvw/Gcw (kg)",55000,55000]
[null,"整备质量(kg) Curb weight(kg)",8870,8870]
[null,"载质量/载人数 Payload/Seats","46000kg/2 人","46000kg/2 人"]
[null,"动力系统 Power system"]
[null,"发动机型号 Engine model","Cummins X15NS6B660","Cummins X15NS6B660"]
[null,"排放 Emission","EURO VI","EURO VI"]
[null,"排量(L) Displacement(L)",14.5,14.5]
[null,"功率(ps)",660,660]
[null,"最大扭矩(N.m/rpm) Max torque(N.m/rpm)","3200/900-1400","3200/900-1400"]
[null,"变速器 Transmission","ZF12TX3221TO，带缓速器ZF12TX3221TO, retarder","ZF12TX3221TO，带缓速器ZF12TX3221TO, retarder"]
[null,"底盘系统 Chassis system"]
[null,"后桥(吨级/速比) Rear axle(Ton/ratio)","10t3.364","10t3.364"]
[null,"车 架(mm) Frame(mm)","225/286x80x(8+L)","225/286x80x(8+L)"]
[null,"悬 架 Suspension","前:2 片板簧,后:3 片板簧 Front: 2 leaf springs.Rear: 3 leaf springs","前:2 片板簧,后:3 片板簧 Front: 2 leaf springs.Rear: 3 leaf springs"]
[null,"轮 胎 Tyre Model","12R22.5","12R22.5"]
[null,"其他配置及性能"]
[null,"最小离地间隙(mm)",250,250]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}