{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":45,"n_cols":4,"rows_kept":45,"cut":false,"hidden":false,"merged":[[0,1,0,2],[1,1,1,2],[2,1,2,2],[3,1,3,2],[4,1,4,2],[5,1,5,2],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[26,1,26,2],[27,1,27,2],[28,1,28,2],[29,1,29,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,1,33,2],[43,1,43,3],[44,0,44,3],[0,0,1,0],[2,0,16,0],[17,0,20,0],[22,0,29,0],[30,0,33,0],[34,0,42,0]]}
["@基本信息","车辆名称",null,"救险车"]
[null,"车辆型号",null," FZB5035XXHFT4C"]
["@基本参数","排放标准",null,"GB18352.6-2016国Ⅵ"]
[null,"燃料种类",null,"柴油"]
[null,"驱动形式",null,"4×4"]
[null,"轴距（mm）",null,3400]
[null," 轴荷",null,"1278/1702,1095/1340"]
[null,"乘坐人数（人）",null,"2+3"]
[null,"最高车速",null,165]
[null,"轮胎数；轮胎规格",null,"4；245/70R16,265/60R18"]
[null,"外形尺寸（长*宽*高)(mm）",null,"5630x1940x2030,2110,2150,2270"]
[null,"后厢体内部尺寸mm",null,"1805*1580*1130"]
[null,"总质量(kg)",null,"2980,2435"]
[null,"整备质量(kg)",null,"2655,2110"]
[null,"接近角/离去角(°)",null,"27.5/19"]
[null,"前悬/后悬（mm）",null,"955/1275"]
[null,"颜色",null,"工程黄"]
["@发动机","型号",null,"4F20TC "]
[null,"企业",null,"北汽福田汽车股份有限公司 "]
[null,"排量(L)",null,"1.981（涡轮增压）"]
[null,"功率（Kw）",null,120]
["@配置分类","分项明细",null,"选项"]
["@底盘配置","ABS+EBD",null,"●"]
[null,"前盘后鼓",null,"●"]
[null,"撞车自动解锁",null,"●"]
[null,"倒车影像",null,"●"]
[null,"定速巡航",null,"●"]
[null,"发动机防盗",null,"●"]
[null,"一键启动",null,"●"]
[null,"8寸彩色液晶显示屏",null,"●"]
["@专用配置","封闭式多舱钢制箱体（侧后上掀门）",null,"●"]
[null,"设备机柜",null,"●"]
[null,"警灯警示系统",null,"●"]
[null,"车内照明系统",null,"●"]
["@选装配置","厢体两侧","两侧选装卷帘门结构","○"]
[null,"铝制厢体","后厢体选择轻质、防腐铝合金箱体","○"]
[null,"内饰","内饰使用小花纹铝板","○"]
[null,"地板","地板铺设大花纹铝板","○"]
[null,"电动绞盘","主体：DC12V,6000磅；快速拆卸装置","○"]
[null,"折叠升降照明系统","升降1.2米，2*150W，系统电压12V，灯电压220V","○"]
[null,"摄像系统","DBS-BW625C13,130万像素，30倍变焦；DBS4GNVR2004MDR,4路4G/GPS（可远程），1T固态硬盘","○"]
[null,"配电柜","NP282815，带空开等","○"]
[null,"车载医药箱","340*245*125，36种","○"]
["@其它配置","尾部拖车钩：带锁"]
["@备注：（1）●代表标准配置、○代表选装配置，—代表无此配置。\n      （2）如有特殊需求，加装设备的高度、质量参数及外观超出公告参数范围需客户上户前自行拆装。"]