{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":31,"n_cols":4,"rows_kept":31,"cut":false,"hidden":false,"merged":[[1,0,1,1],[2,0,2,1],[3,0,3,1],[4,0,4,1],[5,0,5,1],[6,0,6,1],[7,0,7,1],[8,0,8,1],[9,0,9,1],[10,0,10,1],[11,0,11,1],[12,0,12,1],[13,0,13,1],[14,0,14,1],[15,0,15,1],[16,0,16,1],[17,0,17,1],[18,0,18,1],[19,0,19,1],[20,0,29,0],[30,0,37,0],[30,1,37,3]]}
[null,null,"3吨","5吨"]
[null,null,"5088TQZ00-3P0001","5108TQZ00-5P0001"]
["@产品名称",null,"清障车","清障车"]
["@产品型号",null,"BJ5088TQZ-3P","BJ5108TQZ-5P"]
["@底盘型号",null,"欧马可 BJ1088VEJEA-FK","欧马可 BJ1108VFPEG-FK"]
["@总质量(Kg)",null,8275,9995]
["@整备质量(Kg)",null,5760,6650]
["@外形尺寸(mm)",null,"7770×2400×2340","9060×2550×2365"]
["@轴数",null,2,2]
["@轴距(mm)",null,3800,4700]
["@最高车速(Km/h)",null,105,105]
["@轮胎规格",null,"7.5R16LT 14PR/8.25R16LT 14PR","8.25R16LT 14PR"]
["@发动机型号",null,"福田康明斯/F3.8NS6B156","福田康明斯/F3.8NS6B170"]
["@功率(Kw)",null,115,125]
["@排放标准",null,"国六","国六"]
["@接近角/离去角(°)",null,"20/12","18/13"]
["@前悬/后悬（mm）",null,"1130/2470","1130/3050"]
["@后伸（mm）",null,370,180]
["@制动",null,"气压制动/ABS","气压制动/ABS"]
["@空调",null,"电动空调","电动空调"]
["@专用\n装置\n参数","平台尺寸(mm)","5600×2400","6650×2550"]
[null,"平台承载质量（Kg）",3000,5000]
[null,"平台承载面高度（后桥处）(mm)",1000,1130]
[null,"平台伸缩行程(mm)",3400,3400]
[null,"平台与地面最小夹度(°)",11,11.3]
[null,"绞盘额定拉力（KN）",40,50]
[null,"绞盘钢丝绳长度(m)",25,25]
[null,"托臂全伸托举质量（Kg）",1500,2000]
[null,"托臂最大有效长度(mm)","1820（至L臂抱胎中心）","2120（至L臂抱胎中心）"]
[null,"托臂伸缩行程(mm)",1400,1850]
["@产品\n卖点","底盘是福田欧马可专为清障车开发的专用底盘，配有黄金动力传动链，承载能力强，动力强劲。\n平台与地面作业夹角：11度，满足更多车辆拖牵需求。\n平台承载面离地高度同类产品最低。\n平台承载面有效宽度，同类产品最宽。\n平台边框设有长圆孔，更方便被拖车辆的捆绑固定。\n车辆尾部设有活动支脚，路况不佳时收起，车辆通过性更好。\n平台底板下面布设加强矩形管，满足工程机械承载要求。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}