{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[[0,0,0,3],[0,5,0,10],[2,0,8,0],[9,0,13,0],[14,0,15,0],[19,0,22,0],[23,0,25,0]]}
["@行星",{"$nulls":4},"（玉柴）8方、10方、12方城市、12方山区、大12方\n（潍柴）8方、10方、12方山区、大12方"]
["$产品","$型号","&MA405","&MB407","&MC408","&MC408","&MC408","&MA405","&MB407","&MC408","&MC408"]
["@整车参数","@整车型号","BJ5316GJB-MA/BJ5311","BJ5316GJB-MB/BJ5311","BJ5316GJB-MC/BJ5311","BJ5316GJB-MC/BJ5311","BJ5316GJB-MD/BJ5311","BJ5316GJB-MA/BJ5311","BJ5316GJB-MB/BJ5311","BJ5316GJB-MC/BJ5311","BJ5316GJB-MD/BJ5311"]
[null,"@整车尺寸（mm）","9588*2530*3910","9815*2530*3990","9850*2530*3950","9850*2530*3950","9900*2530*3970","9588*2530*3910","9815*2530*3990","9850*2530*3950","9900*2530*3970"]
[null,"@轴距（mm）","2000+2850+1350","2000+2850+1350","2000+2850+1350","2000+2800+1400","2000+2800+1400","2000+2850+1350","2000+2850+1350","2000+2800+1400","2000+2800+1400"]
[null,"@最大总质量（kg）",31000,31000,31000,31000,31000,31000,31000,31000,31000]
[null,"@整备质量（kg）","12150/11500","12550/11600","13700/13400",13700,14000,"12150/11500","12550/11600",13700,14000]
[null,"@额定载质量（kg）",18720,18320,17170,17170,16870,18720,18320,17170,16870]
[null,"@罐体尺寸（mm）","2200*4818","2200*5398","2200*6058","2200*6058","2300*6000","2200*4818","2200*5398","2200*6058","2300*6000"]
["@上装参数","@上装方量（mm³）","B","SH","SE","SE","SE","B","SH","SE","SE"]
[null,"@副车架形式","有副梁","有副梁","有副梁","有副梁","有副梁","有副梁","有副梁","有副梁","有副梁"]
[null,"@清洗方式","气压","气压","气压","气压","气压","气压","气压","气压","气压"]
[null,"@滑料槽举升机构","手摇式","手摇式","手摇式","手摇式","手摇式","手摇式","手摇式","手摇式","手摇式"]
[null,"@爬梯型式","双面斜爬梯","双面斜爬梯","双面斜爬梯","双面斜爬梯","双面斜爬梯","双面斜爬梯","双面斜爬梯","双面斜爬梯","双面斜爬梯"]
["@动力系统","@发动机","YCK08350-60","YCK08350-60","YCK08350-60","YCK08350-60","YCK08350-60","WP8.350E62","WP8.350E62","WP8.350E62","WP8.350E61A"]
[null,"@变速器","10JSD140T","10JSD140T","10JSD140T","10JSD140T","10JSD140T","10JSD140T","10JSD140T","10JSD140T","10JSD140T"]
[null,"@轮胎","11.00R20 18PR  12R22.5 18PR 、11R22.5 18PR","11.00R20 18PR  12R22.5 18PR 、11R22.5 18PR","11.00R20 18PR  12R22.5 18PR 、11R22.5 18PR","11.00R20 18PR  12R22.5 18PR 、11R22.5 18PR","11.00R20 18PR  12R22.5 18PR 、11R22.5 18PR","11.00R20 18PR  12R22.5 18PR 、11R22.5 18PR","11.00R20 18PR  12R22.5 18PR 、11R22.5 18PR","11.00R20 18PR  12R22.5 18PR 、11R22.5 18PR","11.00R20 18PR  12R22.5 18PR 、11R22.5 18PR"]
[null,"@驱动形式","8*4","8*4","8*4","8*4","8*4","8*4","8*4","8*4","8*4"]
[null,"@排放","国Ⅵ","国Ⅵ","国Ⅵ","国Ⅵ","国Ⅵ","国Ⅵ","国Ⅵ","国Ⅵ","国Ⅵ"]
["@搅拌参数","@残余率（%）","≤0.5","≤0.5","≤0.5","≤0.5","≤0.5","≤0.5","≤0.5","≤0.5","≤0.5"]
[null,"@塌落度范围（mm）","120-200","120-200","120-200","120-200","120-200","120-200","120-200","120-200","120-200"]
[null,"@进料速度（m³/min）","≥3","≥3","≥3","≥3","≥3","≥3","≥3","≥3","≥3"]
[null,"@出料速度（m³/min）","≥2","≥2","≥2","≥2","≥2","≥2","≥2","≥2","≥2"]
["@上装配置","@搅拌罐体","T980CGJ","T980CGJ","T980CGJ","T980CGJ","T980CGJ","T980CGJ","T980CGJ","T980CGJ","T980CGJ"]
[null,"@液压系统","标配国产，选配进口","标配国产，选配进口","标配国产，选配进口","标配国产，选配进口","标配国产，选配进口","标配国产，选配进口","标配国产，选配进口","标配国产，选配进口","标配国产，选配进口"]
[null,"@水箱容积（L）","300L 铝合金","300L 铝合金","300L 铝合金","300L 铝合金","300L 铝合金","300L 铝合金","300L 铝合金","300L 铝合金","300L 铝合金"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}